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1. Complete all blanks as indicated.
2. Refer to "Right-of-Way Memo:  Access Control, Board Policy 4005, and IDAPA Rule 39.03.42" for further information.
3. Indicate the units under "Limits" as either Milepost (MP) or Station (Sta.)
4. Provide justification for the proposed limits of Access Purchase. Attach Traffic Impact Study as needed.
5. Attach an 8 1/2" x 11" Vicinity Map showing the limits of purchased access if the limits are not readily understood (e.g., an interchange or major intersection).
6. Complete the ITD 0606 and send a copy to Headquarters Right-of-Way in concurrence with the Right-of-Way plans.
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Types of Access Spacing

Effective December 12, 2012, the Idaho Board approved Board Policy 4005 - Management of Department-Owned Property, which incorporated the recently revised IDAPA Rule 39.03.42 - Rules Governing Right-of-Way Encroachments on State Rights-of-Way.

Under the revised IDAPA Rule 39.03.42, all routes on the State Highway System are classified into one of six tiers; Interstate, Freeway, Expressway, Statewide, Regional, and District.  Segments of highway are further classified according to whether they are rural, transitional, urban high-speed, or urban low-speed.  A map of these classifications is attached to this memo and is available at: September 2012 Access Map.

Any existing access removed during a highway project shall be documented on the right-of-way documents and the "As Constructed" plans.

To maintain system capacity, safety and efficiency, maximize signal progression, and minimize delays to the traveling public, all approaches and signals shall be spaced in accordance with ITD standards.  Variances to the spacing standards shall be handled as follows (from IDAPA 39.03.42):

The District Engineer shall have the authority to approve a decrease in the minimum access spacing distances set forth in Table 1, provided that the basis for any exception is justified and documented. The basis for the exception may include overriding economic opportunity considerations. For any exception that would result in a decrease in access spacing of more than ten percent (10%) of the distances set forth in Table 1, a Traffic Impact Study will be required in order to determine whether auxiliary lanes or other appropriate mitigation must be included in the permit’s conditions. (10-1-12)T 

A copy of this required documentation shall be available in the Project File.

	Idaho Administrative Code
Idaho Transportation Department
	IDAPA 39.03.42 -
	Rules Governing Highway Right-of-Way Encroachments on State Rights-of-Way

	Table 1 – Access Spacing*

	Highway Type
	Area Type
	Signalized Road Spacing
	Public Road Spacing 
(A)
	Driveway Distance Upstream from Public Road Intersection 
(B)
	Driveway Distance Downstream from Unsignalized Public Road Intersection (C)
	Distance Between Unsignalized Accesses Other Than Public Roads (D)

	Interstate
	All
	Accessible only by interchanges (ramps) and requires approval by the Board and Federal Highway Administration

	Freeway
	All
	Accessible only by interchanges (ramps)

	Expressway
	All
	Accessible only at locations specified by the Department

	Statewide Route
	Rural
	5,280 ft.
	5,280 ft.
	1,000 ft.
	650 ft.
	650 ft.

	
	Transitional
	5,280 ft.
	2,640 ft.
	760 ft.
	500 ft.
	500 ft.

	
	Urban >35 mph
	2,640 ft.
	1,320 ft.
	790 ft.
	500 ft.
	500 ft.

	
	Urban <35 mph
	2,640 ft.
	1,320 ft.
	790 ft.
	250 ft.**
	250 ft.**

	Regional Route
	Rural
	5,280 ft.
	2,640 ft.
	1,000 ft.
	650 ft.
	650 ft.

	
	Transitional
	2,640 ft.
	1,320 ft.
	690 ft.
	360 ft.**
	360 ft.**

	
	Urban >35 mph
	2,640 ft.
	660 ft.
	660 ft.
	360 ft.**
	360 ft.**

	
	Urban <35 mph
	2,640 ft.
	660 ft.
	660 ft.
	250 ft.**
	250 ft.**

	District Route
	Rural
	2,640 ft.
	1,320 ft.
	760 ft.
	500 ft.
	500 ft.

	
	Transitional
	2,640 ft.
	660 ft.
	660 ft.
	360 ft.**
	360 ft.**

	
	Urban >35 mph
	1,320 ft.
	660 ft.
	660 ft.
	360 ft.**
	360 ft.**

	
	Urban <35 mph
	1,320 ft.
	660 ft.
	660 ft.
	250 ft.**
	250 ft.**

	*Distances in table are minimums based on optimal operational and safety conditions such as adequate sight distance and level grade. Definitions of spacing designated by (A), (B), (C), and (D) are represented on Figure 1.

	**Where the public road intersection or private access intersection is signalized, the distances in the table are for driveways restricted to right-in/right-out movements only. For unrestricted driveways the minimum distance shall be 500 feet from a signalized intersection.
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