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ITD 1866   (Rev. 8-25)
Cement Recycled Asphalt Base Stabilization (CRABS)
itd.idaho.gov
Density Verification
	Key Number
	Project Number
	Project Name
	District

	     
	     
	     
	     

	Tested By
	Moisture Between 4% and 7%?
	WAQTC Number
	Date Tested

	     
	Yes / No
	     
	     

	Gauge Make
	Gauge Model Number
	Gauge Serial Number

	     
	     
	     


	
	Test Number
	     
	     
	     
	     
	     

	
	Test Date
	     
	     
	     
	     
	     

	Test Location
	Station
	     
	     
	     
	     
	     

	
	Offset
	     
	     
	     
	     
	     

	Uncorrected Densities*
	Pass Number   1
	     
	     
	     
	     
	     

	
	Pass Number   2
	     
	     
	     
	     
	     

	
	Pass Number   3
	     
	     
	     
	     
	     

	
	Pass Number   4
	     
	     
	     
	     
	     

	
	Pass Number   5
	     
	     
	     
	     
	     

	
	Pass Number   6
	     
	     
	     
	     
	     

	
	Pass Number   7
	     
	     
	     
	     
	     

	
	Pass Number   8
	     
	     
	     
	     
	     

	
	Pass Number   9
	     
	     
	     
	     
	     

	
	Pass Number 10
	     
	     
	     
	     
	     

	
	Pass Number 11
	     
	     
	     
	     
	     

	
	Pass Number 12
	     
	     
	     
	     
	     

	
	Pass Number 13
	     
	     
	     
	     
	     

	
	Pass Number 14
	     
	     
	     
	     
	     


*Note: Densities should be run as per WAQTC TM-8 with the following exceptions:


A.  The use of sand as a filler is not required.

B.  Only one reading is required per pass. It is not necessary to turn the gauge 90 degrees and take another reading.

Note: The required compaction is achieved when the final roller pass adds no more than 0.5 lbs/ft3 to the previous in-place density.
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	Remarks

	     


	Reviewed By
	Date

	     
	     


