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[bookmark: _Toc345918710][bookmark: _Toc345919140][bookmark: _Toc478041442]Section 1: SWPPP Framework
[bookmark: _Toc303088769][bookmark: _Toc323128847]
[bookmark: _Toc478041443]Regulatory and Policy Overview

This narrative is a part of the Stormwater Pollution Prevention Plan (SWPPP) and is a requirement of the Idaho Pollutant Discharge Elimination System (IPDES) Construction General Permit for Discharge Activities (CGP). CGP coverage is required from the “Commencement of Earth-Disturbing Activities” and “Commencement of Pollutant-Generating Activities” until “Final Stabilization” as defined in Appendix A of the 2022 CGP.  The SWPPP may reference the following regulations, specifications, protocols, provisions, best management practices (BMPs), and standard drawings including, but not limited to: CGP and referenced Codes of Federal Regulation (CFR) requirements, February 2022; ITD Best Management Practices Manuals, January 2014 as amended; ITD Standard Specifications for Highway Construction; ITD Supplemental Specifications; ITD Special Contract Provisions; ITD Contractor’s Notes, Approved Project Bid Plans; on-site policies adopted and approved by the Engineer during construction; United States Army Corps of Engineers (USACE) 404 permit (if applicable); Idaho Department of Environmental Quality (IDEQ) 401 Certifications (if applicable), Idaho Department of Water Resources (IDWR) Stream Alteration Permit requirements (if applicable), and any change orders that apply.

[bookmark: _Toc303088770][bookmark: _Toc323128848][bookmark: _Toc345918712][bookmark: _Toc345919142][bookmark: _Toc478041444]Notice of Intent and CGP Requirements

To obtain coverage for stormwater discharges under the 2022 CGP, all Operators, including operators of a “Construction Support Activity”, as defined in Appendix A of the CGP, must prepare and submit a complete and accurate Notice of Intent (NOI) which meets CGP Part 1 requirements.  It is the responsibility of all operators to fully understand the information requirements to be provided when filling out a NOI.  Discharges are not authorized if the NOI is incomplete or inaccurate. Authorization to discharge stormwater from construction activities under the terms and conditions of the CGP will be permitted fourteen a minimum of (14) calendar days after the submittal of a complete and accurate NOI is acknowledged on IDEQ’s website, unless IDEQ notifies you that your authorization has been delayed or denied. 

Note: This SWPPP must be finalized and certified by all Operators prior to submittal of NOIs for permit coverage.  Copies of the Idaho Department of Environmental Quality (IDEQ) Notice of Intent (NOI) submittal form and IDEQ NOI acknowledgement from the IPDES E-permitting System notifying the operator of an administratively complete NOI and approved authorization must be included as a component of this SWPPP in Appendix.

[bookmark: _Toc303088771][bookmark: _Toc323128849][bookmark: _Toc345918713][bookmark: _Toc345919143][bookmark: _Toc478041445]Operator Requirements

As an operator, compliance with all applicable terms and conditions of the CGP as it relates to operator controls and activities on the construction site or construction support activities, is the sole responsibility of the operator.  All operators including, but not limited to; project owners or sponsors, Contractors, applicable subcontractors, or any other entity who has operational control over construction plans and specifications, operational control over day-to-day activities, or operational controls within a construction support activity that is a portion of a larger project; must ensure CGP compliance.

[bookmark: _Toc345918714][bookmark: _Toc345919144][bookmark: _Toc478041446]Design Specifications and Requirements

Follow all manufacturers design specifications for the installation and maintenance of controls.  In the absence of specific manufacturer’s specifications, follow ITD standard drawings and the ITD Best Management Practices Manuals.  These can be referenced at itd.idaho.gov.   
For special conditions not covered in the design specifications or ITD guidance materials, consult with the Resident Engineer or ITD SWPPP practitioners to ensure proper application and installation of BMPs.  Many of the commonly used stormwater controls used by ITD are on the Qualified Products List (QPL).  In order for a product to get approved on this list, design specifications are reviewed by a QPL committee.  Therefore, if a QPL approved product is used on this project, and it is installed and maintained properly, it is being utilized per the manufacturer’s design specifications.  The ITD Qualified Products List can be referenced at:
http://apps.itd.idaho.gov/apps/materials/QPL.aspx


[bookmark: _Toc345918715][bookmark: _Toc345919145][bookmark: _Toc478041447]Section 2: Contact Information/Responsible Parties/Stormwater Team Members

Operator(s) - See definition of “Operator” at CGP Part 1.1.1
	Idaho Transportation Department
	SWPPP Developer Name

	
	

	Address
	City
	State
	Zip Code

	
	
	ID
	

	Fax Number
	Telephone Number
	E-Mail Contact

	
	
	



Prime Contractor
	Company or Organization Name
	Name

	
	

	Address
	City
	State
	Zip Code

	
	
	
	

	Fax Number
	Telephone Number
	E-Mail Contact

	
	
	

	Area of Control (if more than one operator at site)

	



Earth Disturbing Subcontractor(s)
	Company or Organization Name
	Name

	
	

	Address
	City
	State
	Zip Code

	
	
	
	

	Fax Number
	Telephone Number
	E-Mail Contact

	
	
	

	Area of Control (if more than one operator at site)

	


Repeat as needed for all additional Earth Disturbing Subcontractors.

Contractor’s Emergency 24-Hour Contact (Water Pollution Control Manager)
	Company or Organization Name
	Name

	
	

	Address
	City
	State
	Zip Code

	
	
	
	

	Fax Number
	Telephone Number
	E-Mail Contact

	
	
	



Stormwater Team - See CGP Part 7.2.2 and Section 6 and SWPPP Section 7.
	Role or Responsibility
	Position
	Name

	
	Agency Stormwater Inspector(s)
	

	City
	State
	Zip Code

	
	ID
	

	Telephone Number
	E-Mail Contact

	
	



	Role or Responsibility
	Position
	Name

	
	Contractor’s WPCM(s)
	

	City
	State
	Zip Code

	
	
	

	Telephone Number
	E-Mail Contact

	
	



	Role or Responsibility
	Position
	Name

	
	Agency Resident Engineer
	

	City
	State
	Zip Code

	
	ID
	

	Telephone Number
	E-Mail Contact

	
	



	Role or Responsibility
	Position
	Name

	Certifier and Signature Authority
	Agency DE or DEM or Equivalent
	

	City
	State
	Zip Code

	
	ID
	

	Telephone Number
	E-Mail Contact

	
	



	Role or Responsibility
	Position
	Name

	Certifier and Signature Authority
	Prime Contractor’s Responsible Corporate Officer
	

	City
	State
	Zip Code

	
	
	

	Telephone Number
	E-Mail Contact

	
	



Describe additional stormwater team members here.  Copy and paste for additional team members. 
	Role or Responsibility
	Position
	Name

	
	
	

	City
	State
	Zip Code

	
	
	

	Telephone Number
	E-Mail Contact

	
	



[bookmark: _Toc323128854][bookmark: _Toc331162601]

[bookmark: _Toc345918716][bookmark: _Toc345919146][bookmark: _Toc478041448][bookmark: _Toc158629988][bookmark: _Toc323128855]Section 3: Site Evaluation, Assessment, and Planning
[bookmark: _Toc331162602]
[bookmark: _Toc345918717][bookmark: _Toc345919147][bookmark: _Toc478041449]3.1  Project/Site Information
	Project/Site Name

	

	Project Street/Location/Address/Mileposts

	

	City
	State
	Zip Code
	County or Similar Subdivision

	
	ID
	
	



Project Latitude/Longitude
	*(Use one of three possible formats: 1) degrees, minutes, seconds; 2) degrees, minutes, decimal; or 3) decimal)

	Latitude: 
	Longitude: 



Specify method for determining latitude/longitude (enter X in box next to appropriate answer)
	[bookmark: Check31]|_| United States Geological Survey (USGS) topographic map (if used, specify scale)
	
	

	[bookmark: Check32]|_| EPA Web site
	[bookmark: Check33]|_| GPS
	[bookmark: Check34]|_| Other (please specify)
	
	

	
	
	
	
	



Horizontal Reference Datum
	[bookmark: Check28]|_| NAD 27
	[bookmark: Check29]|_| NAD 83 or WGS 84
	[bookmark: Check30]|_| Unknown



Additional Project Information
	Is the project/site located on Indian country lands?

	[bookmark: Check35]|_| Yes
	[bookmark: Check36]|_| No

	If yes, STOP FILLING OUT THIS IPDES SWPPP TEMPLATE AND USE THE EPA NPDES SWPPP TEMPLATE. 
THE EPA ADMINISTERS THE NPDES PROGRAM ON TRIBAL LANDS.

	



	If you are conducting earth-disturbing activities in response to a public emergency, document the cause of the public emergency (e.g., natural disaster, extreme flooding conditions), information substantiating its occurrence (e.g., state disaster declaration), and a description of the construction necessary to reestablish effective public services.

	



	Description of Soil Type(s):

	

	Description of Slopes: (describe existing slopes and note any changes due to grading or fill activities)

	

	Description of Drainage Patterns: (describe existing drainage patterns and note any changes dues to grading or fill activities)

	

	Description of existing or baseline vegetation on or immediately surrounding the project area:

	

	Climate/Rainfall Patterns: - check the box that applies

	[bookmark: Check16][bookmark: Check17]|_| Arid (0-10” annual rainfall)	|_| Semi-Arid (10”-20” annual rainfall)

|_| (20-30” annual rainfall)	|_| (30”-40” annual rainfall)

	

Provide a description of unique or sensitive features (such as wetlands) that are to be preserved or protected

	

	Describe measures to protect these unique or sensitive features

	



[bookmark: _Toc323128856][bookmark: _Toc331162603][bookmark: _Toc345918718][bookmark: _Toc345919148][bookmark: _Toc478041450][bookmark: _Toc158629990]3.2  Discharge Information
Note: Information entered here should be consistent with the “Discharge Information” in Section V of the project’s NOI form (CGP Appendix F, and the “NOI” Section of the SWPPP Appendix.)

	
	Yes
	No

	Does your project/site discharge stormwater into a Municipal Separate Storm Sewer System (MS4)? 	
	[bookmark: Check37]|_|
	[bookmark: Check41]|_|

	Does your project have construction support activities that discharge stormwater into a MS4? 	
	[bookmark: Check38]|_|
	[bookmark: Check42]|_|

	Are there any surface waters (Waters of the U.S.) that are located within 50 feet of your construction site disturbances? 	
	[bookmark: Check39]|_|
	[bookmark: Check43]|_|

	Are there any surface waters (Waters of the U.S.) that are located within 50 feet of your construction support activities? 	
	[bookmark: Check40]|_|
	[bookmark: Check44]|_|



Table 1 – Names of Receiving Waters
	List name(s) of the first surface water (Waters of the U.S.) that receives stormwater directly from your project and/or from the MS4 (Note:  multiple rows are provided where your site has more than one point of discharge that flows to different surface waters which is not uncommon on linear transportation projects).  

	

	1.
	

	2.
	

	3.
	

	4.
	


Add additional rows as needed by hitting Tab in the last cell of the table

Table 2 – Impaired Waters / TMDLs 
	For each surface water listed in Table 1 above, answer the following: Is this surface water listed as “Impaired”?  Impaired waters will be on IDEQ’s 303(d) list waiting for an EPA approved TMDL, or already have an EPA approved TMDL.  If your answer is Yes, then provide required information following on that row.

	
	List pollutant(s) that are
	A TMDL has been completed
	Title of the TMDL Document
	Pollutant(s) with a TMDL

	
	Yes
	No
	causing the impairment
	Yes
	No
	
	

	1.
	[bookmark: Check20]|_|
	[bookmark: Check24]|_|
	
	[bookmark: Check45]|_|
	[bookmark: Check46]|_|
	
	

	2.
	[bookmark: Check21]|_|
	[bookmark: Check25]|_|
	
	[bookmark: Check52]|_|
	[bookmark: Check47]|_|
	
	

	3.
	[bookmark: Check22]|_|
	[bookmark: Check26]|_|
	
	[bookmark: Check51]|_|
	[bookmark: Check48]|_|
	
	

	4.
	[bookmark: Check23]|_|
	[bookmark: Check27]|_|
	
	[bookmark: Check50]|_|
	[bookmark: Check49]|_|
	
	


Add additional rows as needed by hitting Tab in the last cell of the table

IDEQ Turbidity Monitoring Requirements
The permittee must conduct turbidity monitoring during construction activities and thereafter on days where there is a direct discharge of pollutants from an unstabilized portion of the site which is causing a visible plume to a water of the United States during operating hours. See CGP Part 3 for more information. Also, see ITD’s Turbidity Monitoring contract Special Provision for additional information regarding monitoring locations and documentation/reporting requirements.  If applicable, insert a copy of these documents, including the monitoring log book documentation (as per the contract Special Provision) into the corresponding SWPPP Appendix.

Table 3 – Tier 2 Waters
For each surface water listed in Table 1 above, answer the following: Is this surface water designated as a Tier 2 water?
Notes:
· There are currently only Tier 1 and Tier 2 waters in Idaho.  No water bodies have been designated as Tier 3 by the Idaho legislature;
· If you listed a water body as impaired in Table 2 above, it is most likely not a Tier 2 water, although IDEQ does retain the authority to determine that a 303(d) listed water body is actually a high quality Tier 2 water.
· Tier 2 waters are fully supporting their designated beneficial uses according to the most recent IDEQ Integrated Report.  See CGP Part 3.2 for more information.

	
	Yes
	No
	If you answered Yes, specify which surface water is designated as Tier 2?

	1.
	[bookmark: Check53]|_|
	[bookmark: Check60]|_|
	

	2.
	[bookmark: Check54]|_|
	[bookmark: Check59]|_|
	

	3.
	[bookmark: Check55]|_|
	[bookmark: Check58]|_|
	

	4.
	[bookmark: Check56]|_|
	[bookmark: Check57]|_|
	



Method Used to Determine Receiving Water Quality Status
	Describe the method(s) you used to determine the status of your receiving waters above.  In Idaho, the options for making this determination are:

|_| IDEQ’s most recent Integrated Report

|_| IDEQ’s Integrated Report Mapping Tool

|_| Written correspondence with your regional IDEQ office to confirm your determination


	Provide additional information or comments below on how this determination was made.  Also see CGP part 9.7.1.

	



[bookmark: _Toc323128857][bookmark: _Toc331162604][bookmark: _Toc345918719][bookmark: _Toc345919149][bookmark: _Toc478041451]3.3  Nature of the Construction Activity
(See CGP Parts 1.2.1.c and 7.2.3)

	General Description of Project

	Provide a general description of the construction project.  (Describe the major phases of construction in SWPPP Section 3.4.)

	



	Size of Construction Project

	Construction Project Size
	Total Area Expected to be Disturbed (Must match area entered in Part IV of the project NOIs)
	Maximum Area Disturbed at Any One Time

	
	
	

	
	
	



	Construction Support Activities (if applicable)
Describe any construction support activities for the project (e.g., concrete or asphalt batch plants, equipment staging yards, material storage areas, excavated material disposal areas, borrow areas) and their associated disturbances to the nearest ¼ acre.  Support Activity disturbances should be added to the Construction Site disturbances to sum up the Total Area Expected to be Disturbed box above.  Repeat as necessary for each applicable support activity and add to the total.


	Construction Support Activity Description

	

	Size of Disturbance for Support Activity
	Support Activity Address or Latitude/Longitude

	
	

	Construction Support Activity Contact Person's Name
	Phone Number
	E-Mail Address

	
	
	


Repeat as needed for additional Support Activity areas or locations.

[bookmark: _Toc323128858][bookmark: _Toc331162605][bookmark: _Toc345918720][bookmark: _Toc345919150][bookmark: _Toc478041452][bookmark: _Toc158629993]3.4  Sequence and Estimated Dates of Construction Activities
(See CGP Part 7.2.3.f for detailed requirements for this SWPPP section)

Note: The Critical Path Method (CPM) schedule on many projects contains detailed information about grading, stabilization, and stormwater control installation practices and associated timelines or phases.  If a CPM is available containing at least the details prompted in this SWPPP section, place it in the “Grading and Stabilization” Activities SWPPP Appendix, in lieu of completing 3.4.

	Phases of Construction - Describe all major phases of construction.

	Phase I

	General Description of Construction Phase - Include estimated area of disturbance associated with this phase.

	

	Estimated Start Date of Disturbances for This Phase
	Estimated End Date of Disturbances for This Phase

	
	

	Stormwater Control(s)
	Estimated Date(s) of Installation
	Estimated Date(s) of Removal

	
	
	

	Structure(s) to be Demolished
	Age of Structure(s)
	Estimated Dates (s) of Demolition

	Stabilization Measures Required
	Estimated Date of Application(s)

	
	


Repeat as needed for all additional construction phases.

[bookmark: _Toc158630003][bookmark: _Toc323128859][bookmark: _Toc331162606][bookmark: _Toc345918721][bookmark: _Toc345919151][bookmark: _Toc478041453][bookmark: _Toc158629998]3.5  Allowable Non-Stormwater Discharges
(See CGP Parts 1.2.2 and 7.2.5)

Notes:
· CGP requirement to identify the likely locations of allowable non-stormwater discharges on the site map(s).
· The most commonly occurring non-stormwater ITD discharges are highlighted below, but others may be present on your project.

	Type of Allowable Non-Stormwater Discharge
	Likely to be Present at This Site

	
	Yes
	No
	

	  1.
	Discharges from emergency fire-fighting activities	
	[bookmark: Check61]|_|
	[bookmark: Check73]|_|
	

	  2.
	Fire hydrant flushings	
	[bookmark: Check62]|_|
	[bookmark: Check74]|_|
	

	  3.
	Landscape irrigation	
	[bookmark: Check63]|_|
	[bookmark: Check75]|_|
	

	  4.
	Waters used to wash vehicles and equipment	
	[bookmark: Check64]|_|
	[bookmark: Check76]|_|
	

	  5.
	Water used to control dust	
	[bookmark: Check65]|_|
	[bookmark: Check77]|_|
	

	  6.
	Potable water including uncontaminated water line flushings	
	[bookmark: Check66]|_|
	[bookmark: Check78]|_|
	

	  7.
	Routine external building wash down	
	[bookmark: Check67]|_|
	[bookmark: Check79]|_|
	

	  8.
	Pavement wash waters	
	[bookmark: Check68]|_|
	[bookmark: Check80]|_|
	

	  9.
	Uncontaminated air conditioning or compressor condensate	
	[bookmark: Check69]|_|
	[bookmark: Check81]|_|
	

	10.
	Uncontaminated, non-turbid discharges of ground water or spring water	
	[bookmark: Check70]|_|
	[bookmark: Check82]|_|
	

	11.
	Foundation or footing drains	
	[bookmark: Check71]|_|
	[bookmark: Check83]|_|
	

	12.
	Construction dewatering water	
	[bookmark: Check72]|_|
	[bookmark: Check84]|_|
	

	

	[bookmark: Check18]Non-stormwater discharges are not applicable to this project   |_|



List allowable non-stormwater discharges using the same number as marked above and the measures used to eliminate or reduce them and to prevent them from becoming contaminated.  Delete the table if “Non-stormwater discharges are not applicable to this project” box is checked above.
	Measures that will be Implemented to Eliminate or Reduce Non-Stormwater Contamination

	
	

	
	

	
	


Add additional rows as needed by hitting Tab in the last cell of the table

[bookmark: _Toc323128860][bookmark: _Toc331162607][bookmark: _Toc345918722][bookmark: _Toc345919152][bookmark: _Toc478041454]3.6  Site Maps
(See CGP Part 7.2.4) 
Insert site maps in “Site Maps” Section SWPPP Appendix.  For most projects, a series of site maps is necessary to meet the minimum CGP mapping requirements and will consist of site maps and SWPPP plan sheets or drawings. Maps must also show construction support activities associated with this project.
[bookmark: _Toc323128861][bookmark: _Toc331162608][bookmark: _Toc345918723][bookmark: _Toc345919153]


[bookmark: _Toc478041455]Section 4:  Documentation Of Compliance With Other Federal Requirements
[bookmark: _Toc158629996][bookmark: _Toc323128862][bookmark: _Toc331162609]
[bookmark: _Toc345918724][bookmark: _Toc345919154][bookmark: _Toc478041456]4.1  Endangered Species Protection
(See CGP Parts 1.1.5, 7.2.9.a, Appendix C, and the “Endangered Species” Section of the SWPPP Appendix.) 

	Eligibility Criterion - Under which criterion listed in CGP Appendix C is the site eligible for coverage under this permit?

	Criterion
	Supporting Documentation



	
[bookmark: Check85]|_| A
	
No ESA-listed species and/or designated critical habitat present in action area.

Using the process outlined in Appendix C of the CGP, you certify that ESA-listed species and designated critical habitat(s) under the jurisdiction of the USFWS or NMFS are not likely to occur in your site’s “action area” as defined in Appendix A of the CGP.

	
[bookmark: Check90]|_| C
	
Discharges not likely to adversely affect ESA-listed species and/or designated critical habitat.

Include the following information in the Endangered Species Documentation Section in the Appendix:

· List the ESA species and/or designated habitat located in your “action area” using the process outlined in Appendix C of the CGP

· Indicate the distance between the site and the listed species and/or designated critical habitat in the action area (in miles); 

· Include the rationale describing specifically how adverse effects to ESA-listed species will be avoided from the discharges and discharge-related activities. You must also include a copy of your site map from your SWPPP showing the upland and in-water extent of your “action area”. 

	
	· 

	
[bookmark: Check91]|_| D
	
Coordination with USFWS and/or NMFS has successfully concluded.

Include the following information in the Endangered Species Documentation Section in the “Endangered Species” Section in the SWPPP Appendix:

· Copies of the correspondence with the participating agencies.

· Basis statement supporting the selection of this criterion should identify whether USFWS or NMFS or both agencies participated in coordination, the field office/regional office(s) providing that coordination, and the date that coordination concluded.



	


[bookmark: Check92]|_| E
	


ESA Section 7 consultation has successfully concluded.

Include the following information in the Endangered Species Documentation Section in the  “Endangered Species” section of the SWPPP Appendix:

· A Biological Opinion from USFWS and/or NMFS that concludes that the action in question (taking into account the effects of your site’s discharges and discharge-related activities) is not likely to jeopardize the continued existence of listed species, nor the destruction or adverse modification of critical habitat;
OR
· A written concurrence from USFWS and/or NMFS with a finding that the site’s discharges and discharge-related activities are not likely to adversely affect ESA-listed species and/or designated critical habitat.


	 
	

	
	



[bookmark: _Toc323128863][bookmark: _Toc331162610][bookmark: _Toc345918725][bookmark: _Toc345919155][bookmark: _Toc478041457]4.2  Historic Preservation
As a state permit, IPDES does not require determination of effect under Section 106.

[bookmark: _Toc323128864][bookmark: _Toc331162611]

[bookmark: _Toc345918726][bookmark: _Toc345919156][bookmark: _Toc478041458]4.3  Safe Drinking Water Act, Underground Injection Control Requirements
(See CGP Part 7.2.8.B and IDAPA 37.03.03-Rules and Minimum Standards for the Construction of Injection Wells)
	Check any or all of the following controls being installed.  If any controls are installed, insert copies of letters, emails, permitting information, or other communication between you and the IDWR into the “Additional Tribal, State, or Local Program” section of the SWPPP Appendix.

	[bookmark: Check102]|_|
	Infiltration trenches (if stormwater is directed to any bored, drilled, driven shaft or dug hole that is deeper than its widest surface dimension, or has a subsurface fluid distribution system)

	[bookmark: Check103]|_|
	Commercially manufactured pre-cast or pre-built proprietary subsurface detention vaults, chambers, or other devices designed to capture and infiltrate stormwater flow

	[bookmark: Check104]|_|
	Drywells, seepage pits, or improved sinkholes (if stormwater is directed to any bored, drilled, driven shaft or dug hole that is deeper than its widest surface dimension, or has a subsurface fluid distribution system)


[bookmark: _Toc303088783][bookmark: _Toc323128865][bookmark: _Toc331162612][bookmark: _Toc158629999]
[bookmark: _Toc345918727][bookmark: _Toc345919157][bookmark: _Toc478041459]4.4  Other Applicable Federal, Tribal, State or Local Programs

	Examples would include, but not be limited to, a project falling within an MS4 permit area, the county requiring a grading permit, additional tribal requirements, or the project has a Section 404 permit for wetlands. Briefly describe these here as documentation in the SWPPP, and insert any additional information or supporting documentation into the “Additional Tribal, State, or Local Program” section of the SWPPP Appendix.

	


[bookmark: _Toc323128866][bookmark: _Toc331162613]



[bookmark: _Toc345918728][bookmark: _Toc345919158][bookmark: _Toc478041460]Section 5:  Erosion and Sediment Controls
[bookmark: _Toc323128867][bookmark: _Toc331162614]
[bookmark: _Toc345918729][bookmark: _Toc345919159][bookmark: _Toc478041461]5.1  Natural Buffers or Equivalent Sediment Controls
(CGP Parts 2.2.1, 7.2.6, and Appendix D)

Are there any surface waters (Waters of the U.S) within 50 feet of the project’s earth disturbances?

[bookmark: Check105]|_| No - If No, no further documentation is required for this section.  Delete information until SWPPP Section 5.2 below.

[bookmark: Check106]|_| Yes - If Yes, check the Compliance Alternative or applicable Buffer Exception(s) below that has been chosen.  To condense this section, once applicable sections are checked, delete non-applicable sections.

Note: Because of the linear nature of ITD projects, the answers/conditions to the Buffer Alternatives and/or Buffer Exceptions may change multiple times along a project’s limit.  This may make multiple evaluations necessary for some projects.  If applicable, specify the locations of the different evaluations and conclusions by mile-marker or stationing.

Buffer Compliance Alternatives – Choose one of three
	
[bookmark: Check107]|_|
	
A 50-foot undisturbed natural buffer will be provided, as per the requirements in CGP - Appendix D, D.2.3


	
|_|
	An undisturbed natural buffer that is less than 50 feet and supplemented by erosion and sediment controls, achieving the sediment load reduction equivalent to a 50-foot undisturbed natural buffer, will be provided and maintained, as per the requirements in CGP - Appendix D, D.2.3 & D.2.4. 


	|_|
	It is infeasible to provide and maintain an undisturbed natural buffer of any size.  Erosion and sediment controls to achieve the sediment load reduction equivalent to a 50-foot undisturbed natural buffer will be implemented, as per the requirements in CGP – Appendix D., D.2.4, Table D-4.  



Buffer Exceptions – Choose any that apply.
*Note: If multiple exceptions apply to one portion of the project, or different exceptions apply to different portions of the project, specify by mile-marker or stationing.
	
|_|





|_|





|_|




|_|
	
The disturbances within 50 feet of a water of the U.S. include one of the conditions below.  Therefore, are exempt from the requirements Part 2.2.1 and CGP Appendix D:
· Construction approved under a CWA Section 404 permit; or
· Construction of a water-dependent structure or water access areas (e.g., pier, boat ramp, trail). 

There is no discharge of stormwater to waters of the U.S. through the area between the disturbed portions of the site and any waters of the U.S. located within 50 feet of your site.  This includes situations where you have implemented controls measures, such as a berm or other barrier that will prevent such discharges.
· Note - If this exception applies, no further documentation is required for Section 5.1.

No natural buffer exists due to preexisting development disturbances that occurred prior to the initiation of planning for this project.  If disturbing portions of preexisting development, provide justification and documentation.
· Note  - Where some natural buffer exists, but portions of the area within 50 feet of the surface water are occupied by preexisting development disturbances, the site must still comply with one of the CGP Part 2.2.1.a compliance alternatives.

For a “linear project” (defined in Appendix A), site constraints (e.g., limited right-of-way) make it infeasible for me to meet any of the CGP Part 2.2.1.a compliance alternatives.  Include documentation for the following:

· Justification for not meeting one of the buffer compliance alternatives.
· Buffer width retained and/or supplemental erosion and sediment controls to treat discharges to the surface water.

	





[bookmark: _Toc323128868][bookmark: _Toc331162615][bookmark: _Toc345918730][bookmark: _Toc345919160][bookmark: _Toc478041462]5.2  Perimeter Controls
	Insert a general description of how you will comply with CGP Part 2.2.3 and 7.2.6

	



	Perimeter Control 1	Approximate Installation Date or Phase
	
	

	
	
	

	Describe the perimeter control to be installed. Indicate specific controls that will be installed and made operational prior to earth disturbance. 

	

	Insert maintenance requirements for the perimeter control.  At a minimum, CGP Part 2.2.3.a requires removal of sediment "before it has accumulated to one-half of the above-ground height of any perimeter control."

	


Repeat as needed for individual specific perimeter controls.
[bookmark: _Toc323128869][bookmark: _Toc331162616]
[bookmark: _Toc345918731][bookmark: _Toc345919161][bookmark: _Toc478041463]5.3  Sediment Track-Out
	Insert a general description of how you will comply with CGP Part 2.2.4.

	



	Track-Out Control 1	Approximate Installation Date or Phase
	
	

	

	Describe the track-out control to be installed.

	

	At a minimum, you must provide for maintenance that meets the requirement in CGP Part 2.2.4.d. 

	


Repeat as needed for additional individual track-out controls.

[bookmark: _Toc323128870][bookmark: _Toc331162617][bookmark: _Toc345918732][bookmark: _Toc345919162][bookmark: _Toc478041464]5.4  Stockpiled Sediment or Soil
	Insert a general description of how you will comply with CGP Part 2.2.5 and 7.2.6

	



	Stockpile Control 1	Approximate Installation Date or Phase
	
	

	

	Describe the stockpile control to be installed

	

	Insert maintenance requirements for the stockpile control.  At a minimum, you must comply with following requirement in CGP Part 2.2.5 Do not hose down or sweep soil or sediment accumulated on pavement or other impervious surfaces into any stormwater conveyance (unless connected to a sediment basin, sediment trap, or similarly effective control), storm drain inlet, or surface water.

	


Repeat as needed for additional individual stockpile controls.

[bookmark: _Toc323128871][bookmark: _Toc331162618][bookmark: _Toc345918733][bookmark: _Toc345919163][bookmark: _Toc478041465]5.5  Minimize Dust
	Insert a general description of how you will comply with CGP Part 2.2.6 and 7.2.6

	



	Dust Control 1	Approximate Installation Date or Phase
	
	

	

	Describe the dust control to be installed or implemented

	

	Insert maintenance requirements for the dust control

	


Repeat as needed for additional individual dust controls.

[bookmark: _Toc323128872][bookmark: _Toc331162619][bookmark: _Toc345918734][bookmark: _Toc345919164][bookmark: _Toc478041466]5.6  Minimize the Disturbance of Steep Slopes
	Insert a general description of how you will comply with CGP Part 2.2.7 and 7.2.6.  If infeasible, explain why.

	



	Steep Slope Control 1	Approximate Installation Date or Phase
	
	

	

	If steep slope disturbance is required, describe the controls that will be implemented to minimize erosion.  This could include installation of standard erosion and sediment controls, phasing, using stabilization practices, etc.

	

	Insert maintenance requirements for any steep slope controls used.

	


Repeat as needed for additional individual steep slope controls.

[bookmark: _Toc323128873][bookmark: _Toc331162620][bookmark: _Toc345918735][bookmark: _Toc345919165][bookmark: _Toc478041467]5.7  Preservation of Topsoil
	Insert a general description of how you will comply with CGP Part 2.2.8 and 7.2.6.  If infeasible, explain why.

	



	Topsoil Control 1	Approximate Installation Date or Phase
	
	

	

	Describe the topsoil management practices to be implemented. 

	

	Insert maintenance requirements for any the topsoil management practices.

	


[bookmark: _Toc323128874][bookmark: _Toc331162621][bookmark: _Toc345918736][bookmark: _Toc345919166]Repeat as needed for additional individual topsoil preservation controls.

[bookmark: _Toc478041468]5.8  Minimize Soil Compaction
	Insert a general description of how you will comply with CGP Part 2.2.9 and 7.2.6

	



	Soil Compaction Control 1	Approximate Installation Date or Phase
	
	

	

	Describe the soil compaction minimization practices to be utilized where infiltration practices or final vegetation occur

	

	Insert maintenance requirements for any soil compaction minimization practices.

	


Repeat as needed for individual soil compaction controls.

[bookmark: _Toc323128875][bookmark: _Toc331162622][bookmark: _Toc345918737][bookmark: _Toc345919167][bookmark: _Toc478041469]5.9  Storm Drain Inlets
	Insert a general description of how you will comply with CGP Part 2.2.10 and 7.2.6

	



	Storm Drain Inlet Control 1	Approximate Installation Date or Phase
	
	

	

	Describe the storm drain inlet control to be installed

	

	Insert maintenance requirements for the storm drain inlet control.  At a minimum, you must comply with following requirement in CGP Part 2.2.10: “Clean, or remove and replace, the protection measures as sediment accumulates, the filter becomes clogged, and/or performance is compromised.  Where there is evidence of sediment accumulation adjacent to the inlet protection measure, you must remove the deposited sediment by the end of the same work day in which it is found or by the end of the following work day if removal by the same work day is not feasible.”

	


Repeat as needed for individual storm drain inlet controls.

[bookmark: _Toc323128876][bookmark: _Toc331162623][bookmark: _Toc345918738][bookmark: _Toc345919168][bookmark: _Toc478041470]5.10  Constructed Stormwater Conveyance Channels
	Insert a general description of how you will comply with CGP Part 2.2.11 and 7.2.6

	



	Conveyance Channel Control 1	Approximate Installation Date or Phase
	
	

	

	Describe the stormwater conveyance channel control design to be in compliance with 2.1.3.1

	

	Insert maintenance requirements for the stormwater conveyance channels

	


[bookmark: _Toc323128877][bookmark: _Toc331162624]Repeat as needed for individual conveyance channel controls.

[bookmark: _Toc345918739][bookmark: _Toc345919169][bookmark: _Toc478041471]5.11  Sediment Basins
	Insert a general description of how you will comply with CGP Part 2.2.12 and 7.2.6.  If you have determined that it is infeasible to utilize an outlet structure that discharges from the surface (surface discharge is a new requirement in 2017 CGP), provide an explanation for why this is the case.

	



	Sediment Basin Control 1	Approximate Installation Date or Phase
	
	

	

	Describe the sediment basin control to be installed.  Sediment basins are engineered structures and must be developed by a Professional Engineer.  Include any site specific basin designs in the SWPPP plan sheets. 

	

	Insert maintenance requirements for the sediment basin control.  At a minimum, you must comply with following requirement in CGP Part 2.2.12 (f) “Remove accumulated sediment to maintain at least one-half of the design capacity and conduct all other appropriate maintenance to ensure the basin or impoundment remains in effective operating condition.”

	


Repeat as needed for individual sediment basin controls.

[bookmark: _Toc323128878][bookmark: _Toc331162625][bookmark: _Toc345918740][bookmark: _Toc345919170][bookmark: _Toc478041472]5.12  Chemical Treatment
(See CGP Parts 2.2.13 and 7.2.6)

Note: Active treatment will be used on a very small percentage of ITD projects, typically in District 1.  Delete if unused. 

Soil Types
	List all the soil types (including soil types expected to be found in fill material) that are expected to be exposed during construction and that will be discharged to locations where chemicals will be applied

	



Treatment Chemicals
	List all treatment chemicals that will be used at the site and explain why these chemicals are suited to the soil characteristics

	

	Describe the dosage of all treatment chemicals you will use at the site or the methodology you will use to determine dosage

	

	Provide information from any applicable Material Safety Data Sheets (MSDS)

	

	Describe how each of the chemicals will stored

	

	Include references to applicable state or local requirements affecting the use of treatment chemicals, and copies of applicable manufacturer’s specifications regarding the use of your specific treatment chemicals and/or chemical treatment systems

	



Special Controls for Cationic Treatment Chemicals (if applicable)
	If you have been authorized by your applicable Regional Office to use cationic treatment chemicals, include the official EPA authorization letter or other communication.  Identify the specific controls and implementation procedures you are required to implement to ensure that your use of cationic treatment chemicals will not lead to a violation of water quality standards.

	



Schematic Drawings of Stormwater Controls/Chemical Treatment Systems
	Provide schematic drawings of any chemically-enhanced stormwater controls or chemical treatment systems to be used for application of treatment chemicals

	





Training
	Describe the training that personnel who handle and apply chemicals have received prior to permit coverage, or will receive prior to the use of treatment chemicals

	


[bookmark: _Toc323128879][bookmark: _Toc331162626]
[bookmark: _Toc345918741][bookmark: _Toc345919171][bookmark: _Toc478041473]5.13  Dewatering Practices (Typically determined by the Contractor and approved by ITD)
	Insert a general description of how you will comply with CGP Part 2.4 and 7.2.6

	



	Dewatering Practice 1	Approximate Installation Date or Phase
	
	

	

	Describe the dewatering practice to be installed.  If dewatering is required, a site specific dewatering plan is typically developed.  Describe this detailed plan here, or insert into the corresponding SWPPP Appendix. 

	

	Insert discharge and maintenance requirements for each dewatering practice.  At a minimum, you must comply with  the requirement in CGP Part 2.4

	


Repeat as needed for individual dewatering practices.

[bookmark: _Toc323128880][bookmark: _Toc331162627][bookmark: _Toc478041474][bookmark: _Toc345918742][bookmark: _Toc345919172]5.14  Additional Stormwater Controls
(Delete if not used)
	Insert a general description of the problem this control is designed to address.

	



	Control 1	Approximate Installation Date or Phase
	
	

	

	Describe the stormwater control practice to be installed

	

	Insert maintenance requirements for the stormwater control practice

	


Repeat as needed for individual stormwater control practices.

[bookmark: _Toc323128881][bookmark: _Toc331162628][bookmark: _Toc345918743][bookmark: _Toc345919173][bookmark: _Toc478041475]5.15  Project Stabilization Practices
(See CGP Parts 2.2.14, 7.2.3.f.iii, and 7.2.6.b.vi)
Notes:
· Shortened stabilization requirements (7 days instead of 14 days per 2.2.14.c) may apply to the project if you’ve determined that your receiving water(s) is Impaired or Tier 2 in SWPPP Section 3.2.
· This section should be consistent with the summary of stabilization practices by each construction phase as previously summarized in SWPPP Section 3.4.
· Provide the estimated installation date, or phase of construction the stabilization practice will be implemented.  Provide the detailed timing of grading and associated stabilization activities as they occur during construction in the Grading and Stabilization Log found in the Appendix.

Use this table if you are NOT located in an arid, semi-arid, or drought- stricken area. 

	Specific Site Stabilization Practice 

	[bookmark: Check115]|_| Vegetative
	[bookmark: Check116]|_| Non-Vegetative
	[bookmark: Check117]|_| Temporary
	[bookmark: Check118]|_| Permanent

	Installation Phase or Approximate Installation Date
	
	

	

	Describe the site stabilization practice to be installed and how it will meet the requirements of CGP Part 2.2.14 a. and b.

	

	Insert maintenance requirements for the stabilization practice

	


Repeat as needed for all additional site stabilization practices and/or construction phases.

Use this table if you ARE located in an arid, semi-arid, or drought- stricken area. 

	Specific Site Stabilization Practice 

	[bookmark: Check119]|_| Vegetative
	[bookmark: Check120]|_| Non-Vegetative
	[bookmark: Check121]|_| Temporary
	[bookmark: Check122]|_| Permanent

	For vegetative stabilization in arid or semi-arid areas, describe the site conditions, including seasonal dry period dates.

	

	Date Seasonal Dry Period Begins
	
	Date Seasonal Dry Period Ends
	
	

	Installation Phase or Approximate Installation Date
	
	

	

	Describe the site stabilization practice to be installed.  Note how the design will meet the requirements of CGP Part 2.2.14. a and b.

	

	Insert maintenance requirements for the stabilization practice.

	


Repeat as needed for all additional site stabilization practices and/or construction phases.
[bookmark: _Toc158630001]Stabilization Delays Due to Unforeseen Circumstances
Note: You will not be able to include this information in your initial SWPPP.
Use this table only if uncontrollable circumstances have delayed the initiation or completion of a stabilization practice such as those described in CGP Part 2.2.14.a
	Site Stabilization Practice Being Delayed

	[bookmark: Check123]|_| Vegetative
	[bookmark: Check124]|_| Non-Vegetative
	[bookmark: Check125]|_| Temporary
	[bookmark: Check126]|_| Permanent



Justification
	Describe the circumstances that prevent you from meeting the deadlines required in CGP Parts 2.2.14. a and b. and the schedule you will follow for initiating and completing stabilization.

	


Repeat as needed for any additional project stabilization delays.
Additional Note:
[bookmark: _Toc323128882][bookmark: _Toc331162629]The Critical Path Method (CPM) schedule on many projects contains additional information on grading, stabilization, and stormwater control installation practices and timelines.  The CPM schedule should be inserted in the “Grading and Stabilization Activities Log” section of the SWPPP Appendix, if applicable.



[bookmark: _Toc345918744][bookmark: _Toc345919174][bookmark: _Toc478041476]Section 6:  Pollution Prevention – Good Housekeeping Standards
All staging areas, material storage/stockpile sites, source sites (excluding commercial sources), disposal/excess material/ waste sites, haul roads, temporary roads, construction entrances and exits must be approved by the Resident Engineer and have BMPs implemented prior to approved use. The contractor shall not encroach into or affect any cultural resources, endangered species or critical habitat, regulated wetlands and waters of the United States, or other environmentally sensitive areas. Attach a record of Environmental Clearance/Approval for any Contractor designated sites, including cultural/historical resources and Endangered Species Act into the corresponding SWPPP Appendix.

[bookmark: _Toc323128883][bookmark: _Toc331162630][bookmark: _Toc345918745][bookmark: _Toc345919175][bookmark: _Toc478041477]6.1  Potential Sources of Pollution
(See CGP Part 7.2.3.g)
Description of Construction Site Pollutants 
	Pollutant-Generating Activity
	Pollutants or Pollutant Constituents
that could be discharged if exposed to stormwater
	Location on Site 
or reference SWPPP site map where this is shown

	
	
	

	
	
	


Add additional rows as needed

[bookmark: _Toc323128884][bookmark: _Toc331162631][bookmark: _Toc345918746][bookmark: _Toc345919176][bookmark: _Toc478041478]6.2  Spill Prevention and Response
(See CGP Parts 2.3.6 and 7.2.6.b.vii)

All ITD projects shall follow the Idaho Hazardous Materials/WMD Incident Command and Response Support Plan and ITD Incident Management Plan. In addition, a project specific Spill Plan shall be provided by the Contractor, and should be included here, or added to this SWPPP as an additional appendix.
	Insert project specific spill plan and response procedures if applicable.

	


[bookmark: _Toc323128885][bookmark: _Toc331162632]
Contractor should provide spill response and cleanup kits on all projects, and make all appropriate staff aware of their locations. The location of these kits should also be marked on the SWPPP maps or plan sheets.

When/where a release of a hazardous materials in an amount equal to or in excess of a reportable quantity occurs during a 24-hour period as established in accordance with the CGP and Codes of Federal Regulation requirements under either 40 CFR Part 110, 40 CFR Part 117, or 40 CFR Part 302, the finding party must immediately notify the Resident Engineer upon discovery. The Resident Engineer in return will contact the National Response Center (1-800-424-8802) as well as the Idaho Communication Center (1-800-632-8000).

Per IDEQ’s 401 Certification of the 2017 CGP, the following requirements also apply.
· Any spill of hazardous materials must be immediately reported to the appropriate DEQ regional office per (IDAPA 58.01.02.850.03).
· Spills of petroleum products that exceed 25 gallons or that cause a visible sheen on nearby surface waters should be reported to DEQ within 24-hours. 
· Petroleum product spills of less than 25 gallons or spills that do not cause a sheen on nearby surface waters shall only be reported to DEQ if clean-up cannot be accomplished within 24-hours (IDAPA 58.01.02.851.04).

Outside of regular business hours, qualified spills should be reported to the State Communications Center at 1-800-632-8000 or 208-846-7610

[bookmark: _Toc345918747][bookmark: _Toc345919177][bookmark: _Toc478041479]6.3  Fueling and Maintaining Equipment or Vehicles
(See CGP Parts 2.3.1 and 7.2.6.b.vii)
	Insert a general description of how you will comply with the CGP Part 2.3.1 requirement to provide an effective means of preventing and eliminating the discharge of spilled or leaked chemicals, including fuel, from the area where these activities will take place.

	



	Fueling and Maintenance Practice 1   	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practice to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for this pollution prevention practice.

	


[bookmark: _Toc323128886][bookmark: _Toc331162633]
[bookmark: _Toc345918748][bookmark: _Toc345919178][bookmark: _Toc478041480]6.4  Washing Equipment and Vehicles
(See CGP Part 2.3.2) 
	Insert a general description of how you will comply with CGP Part 2.3.2.

	




	Washing/Cleaning Practice 1	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practice to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for this pollution prevention practice.

	


[bookmark: _Toc323128887][bookmark: _Toc331162634]
[bookmark: _Toc345918749][bookmark: _Toc345919179][bookmark: _Toc478041481]6.5  Storage, Handling, and Disposal of Construction Products, Materials, and Wastes
(See CGP Parts 2.3.3. and 7.2.6.b.vii)
[bookmark: _Toc478041482]6.5.1  Building Products - Examples include: asphalt sealants, copper flashing, roofing materials, adhesives, concrete admixtures
	Insert a general description of how you will comply with CGP Part 2.3.3.a

	



	Handling/Storage/Disposal 1 	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practices to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for this pollution prevention practice.

	


Repeat as needed for individual pollution prevention practices.

[bookmark: _Toc478041483]6.5.2  Pesticides, Herbicides, Insecticides, Fertilizers, and Landscape Materials
	Insert a general description of how you will comply with CGP Part 2.3.3.b

	



	Handling/Storage/Disposal 1	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practice to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for this pollution prevention practice.

	


Repeat as needed for individual pollution prevention practices.

[bookmark: _Toc478041484]6.5.3  Diesel Fuel, Oil, Hydraulic Fluids, Other Petroleum Products, and Other Chemicals
	Insert a general description of how you will comply with CGP Part 2.3.3.c

	



	Handling/Storage/Disposal 1	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practice to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for the pollution prevention practice

	


Repeat as needed for individual pollution prevention practices.

[bookmark: _Toc478041485]6.5.4  Hazardous or Toxic Waste
(Examples include paints, solvents, petroleum-based products, wood preservatives, additives, curing compounds, acids.)
	Insert a general description of how you will comply with CGP Part 2.3.3.d

	



	Handling/Storage/Disposal 1	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practice to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for the pollution prevention practice

	


Repeat as needed for individual pollution prevention practices.

[bookmark: _Toc478041486]6.5.5  Construction and Domestic Waste
(Examples include packaging materials, scrap construction materials, masonry products, timber, pipe and electrical cuttings, plastics, Styrofoam, hardened concrete, and other trash or building materials.)
	Insert a general description of how you will comply with CGP Part 2.3.3.e

	



	Handling/Storage/Disposal 1	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practice to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for the pollution prevention practice.

	


Repeat as needed for individual pollution prevention practices.

[bookmark: _Toc478041487]6.5.6  Sanitary Waste
	Insert a general description of how you will comply with CGP Part 2.3.3.f.

	



	Sanitary Waste Practice 1	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practice to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for the pollution prevention practice.

	


[bookmark: _Toc323128888][bookmark: _Toc331162635]Repeat as needed for individual pollution prevention practices.

[bookmark: _Toc345918750][bookmark: _Toc345919180][bookmark: _Toc478041488]6.6  Washing Applicators and Containers used for Paint, Concrete or Other Materials
(See CGP Parts 2.3.4 and 7.2.6.b.vii)

	Insert a general description of how you will comply with CGP Part 2.3.4

	



	Washing/Disposal Practice 1	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practice to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for the pollution prevention practice

	


[bookmark: _Toc323128889][bookmark: _Toc331162636]Repeat as needed for individual pollution prevention practices.

[bookmark: _Toc345918751][bookmark: _Toc345919181][bookmark: _Toc478041489]6.7  Fertilizers
(See CGP Parts 2.3.5 and 7.2.6.b.ix)
	Insert a general description of how you will comply with CGP Part 2.3.5

	



	Pollution Prevention Practice 1	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practice to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for the pollution prevention practice

	


[bookmark: _Toc323128890][bookmark: _Toc331162637]Repeat as needed for individual pollution prevention practices.

[bookmark: _Toc478041490][bookmark: _Toc345918752][bookmark: _Toc345919182]6.8  Additional Pollution Prevention Practices
(Delete if not used)
	Insert a general description of the problem this control is designed to address.

	



	Practice 1	Approximate Installation Date or Phase
	
	

	

	Describe the pollution prevention practice to be installed. If applicable, include copies of the design specifications.

	

	Insert maintenance requirements for the pollution prevention practice

	


[bookmark: _Toc158630005][bookmark: _Toc323128891][bookmark: _Toc331162638]Repeat as needed for individual pollution prevention practices.



[bookmark: _Toc345918753][bookmark: _Toc345919183][bookmark: _Toc478041491]Section 7:  Inspections, Corrective Actions, SWPPP Modifications, and Violation Reporting
[bookmark: _Toc158630006][bookmark: _Toc323128892][bookmark: _Toc331162639]
[bookmark: _Toc345918754][bookmark: _Toc345919184][bookmark: _Toc478041492]7.1  Inspection Personnel and Procedures

On ITD projects, the ITD environmental inspector and the Contractor’s Water Pollution Control Manager are responsible for stormwater compliance inspections and SWPPP implementation and recordkeeping.  These members of the Stormwater Team are listed in SWPPP Section 2.

Form ITD 2802, Stormwater Compliance Inspection, and the accompanying Instructions and Inspection Procedures, provide detailed information on roles and responsibility, as well as inspection procedures.  Include a copy of the most recent version of these ITD documents in the corresponding SWPPP Appendix for reference.  

Inspection Schedule
	Insert project inspection schedule based on CGP Parts 4.2, 4.3, or 4.4, whichever applies.  This may change throughout the lifetime of the project.  Document the updated frequency here for each change, including the date of the change, and include the record of each certified SWPPP modification for these changes in the Appendix.    

	1.

	2.

	3.

	4.

	5.


Repeat as needed for any additional frequency changes.

Projects Normal Work Schedule/Working Hours
	Insert project work schedule in days and hours based on requirement to inspect during projects normal working hours in CGP Parts 4.2, 4.3, or 4.4.  This may change throughout the lifetime of the project.  Document the updated work schedule here for each major change, including the dates of the changes.  Also include the record of each major work schedule change as a certified SWPPP modification record in the corresponding SWPPP Appendix.

	Normal Work Schedule
	Applicable Dates 

	1.
	

	2.
	

	3.
	

	4.
	



Reductions in Inspection Frequency (if applicable)

For Stabilized Areas:
	For the reduction in inspections resulting from stabilization, specify the location and completion dates of stabilization steps (see CGP Part 4.4.1).  It is likely that you will not be able to include this in your initial SWPPP.  These stabilized areas should match what is being documented in the Grading and Stabilization Activities Log in corresponding SWPPP Appendix.

	Location Where Stabilization Steps Have Been Completed
	Applicable Dates 

	1.
	

	2.
	

	3.
	

	4.
	


Repeat as needed for any additional stabilized areas.



Increase in Inspection Frequency for Dewatering

Dewatering discharges:
	Indicate locations for dewatering discharges that will require daily inspections and the approximate dates that discharges will begin and end.

	Location Where Dewatering Will Be Discharged
	Applicable Dates 

	1.
	

	2.
	

	3.
	

	4.
	



For Arid, Semi-Arid Areas or Drought-Stricken Areas – N/A |_|
	For the reduction in inspection frequencies in arid, semi-arid, or drought-stricken areas, insert beginning and ending dates of the seasonally dry period on your site.  It is likely that you will not be able to include this in your initial SWPPP.  If you qualify for this inspection frequency reduction (see CGP Part 4.4.2), document in the inspection frequency table above, and you will need to modify your SWPPP to include this information.

	Beginning Date of Seasonally Dry Period
	
	Ending Date of Seasonally Dry Period
	
	

	
	
	
	



For Frozen Conditions – N/A |_|
	For the reduction in inspections due to 3 months (minimum) of continuously frozen conditions, insert beginning and ending dates of the frozen period for your site. It is likely that you will not be able to include this in your initial SWPPP.  If you qualify for this inspection frequency reduction (see CGP Part 4.4.3), document in the inspection frequency table above, and you will need to modify your SWPPP to include this information.

	Beginning Date of Frozen Period
	
	Ending Date of Frozen Period
	
	

	
	
	
	


Repeat as needed for multiple construction season frozen periods.

Rain Gauge Location and Information (See CGP Part 4.2.2, 4.3, or 4.4)
	Specify location(s) of rain gauge to be used for determining whether a rain event of 0.25 inches or greater has occurred.  If using information from a web-based station representative of your project location, provide the information for that station.

	


[bookmark: _Toc323128893][bookmark: _Toc331162640]
[bookmark: _Toc345918755][bookmark: _Toc345919185][bookmark: _Toc478041493]7.2  Corrective Actions
	Describe the procedures for taking corrective action in compliance with CGP Part 5 and 7.2.7

	Procedures for completing Corrective Actions and associated recordkeeping requirements are described in ITDs 2802 Instructions and Inspection Procedures and in the Construction General Permit contract Special Provision for this project.  See corresponding SWPPP Appendices for required documentation, recordkeeping, and signatory records.  



[bookmark: _Toc345918756][bookmark: _Toc345919186][bookmark: _Toc478041494]7.3  SWPPP Modifications
	Describe the procedures for making SWPPP Modifications in compliance with CGP Part 7.4

	Procedures for completing SWPPP Modifications and associated recordkeeping requirements are described in ITDs 2802 Instructions and Inspection Procedures and in the Construction General Permit contract Special Provision for this project.  See corresponding Appendices for processes and procedures for making SWPPP Modifications, required documentation, recordkeeping, and signatory records.  


[bookmark: _Toc158630007][bookmark: _Toc323128894][bookmark: _Toc331162641]
[bookmark: _Toc478041495]




7.4  Reportable CGP Violations
	CGP Part 9.12 and Part 5 include information describing CGP noncompliance reporting requirements.  On ITD projects, the contract documents specify that the Contractor’s Water Pollution Control Manager is required to provide verbal notification to the Engineer immediately when a reportable violation occurs, and within 24 hours in writing using the ITD Form 2790. Insert a copy of written Notice of Potential Violation into the corresponding SWPPP Appendix.  



[bookmark: _Toc345918757][bookmark: _Toc345919187][bookmark: _Toc478041496]7.5  Delegation of Authority
	On ITD projects, all Operators who file a Notice of Intent must certify the project SWPPP in Section 9.  CGP Part 9 includes detailed information regarding signatory requirements.  If the person who will be signing inspection reports, corrective action reports, and SWPPP modifications is different than the person who certified the original SWPPP in Section 9, insert a copy of the completed and signed delegation of authority form into the corresponding SWPPP Appendix. 






[bookmark: _Toc158630009][bookmark: _Toc323128895][bookmark: _Toc331162642][bookmark: _Toc345918758][bookmark: _Toc345919188][bookmark: _Toc478041497]Section 8:  Recordkeeping and Training
[bookmark: _Toc323128896][bookmark: _Toc331162643]
[bookmark: _Toc345918759][bookmark: _Toc345919189][bookmark: _Toc478041498]8.1  Training Requirements
(See CGP Part 6)

On ITD projects, the ITD Environmental Inspector(s) must have a current NPDES Inspector Qualification based on completion of ITD courses 3.07 or 3.09, the NPDES Stormwater for Construction Staff/Inspector Initial Qualification Course or its subsequent Refresher Course.   

The Contractor’s WPCM(s) must have a current Water Pollution Control Manager Qualification based on attendance of an ITD approved, AGC provided WPCM course, or EPA.    

Both these training courses meet the staff training requirement of CGP Part 6, and the Qualified Person as defined in CGP Part 6.3.  Insert certificates documenting course completion into the SWPPP Appendix.

You are not required to provide or document formal training for subcontractors or other outside service providers, but must ensure that such personnel understand any requirements of the permit that may be affected by the work they are subcontracted to perform.  If informal training, or tailgate trainings are completed and you’d like to document their completion, complete the ITD Form 2958 and include a copy in the SWPPP Appendix. 
[bookmark: _Toc323128897][bookmark: _Toc331162644][bookmark: _Toc158630013]
[bookmark: _Toc345918760][bookmark: _Toc345919190][bookmark: _Toc478041499]8.2  Construction General Permit

Insert a complete copy of the 2022 Construction General Permit in the SWPPP Appendix.  Use two sided printing to minimize space.
[bookmark: _Toc323128898][bookmark: _Toc331162645]
[bookmark: _Toc345918761][bookmark: _Toc345919191][bookmark: _Toc478041500]8.3  Notice of Intent and IDEQ Acknowledgment Letters

ITD, the Contractor, and any applicable local or 3rd party Operator filing an NOI should include a copy of their complete Notice of Intent, IDEQ Acknowledgment Letters, as well as Notices of Termination (NOTs) in the SWPPP Appendix.

[bookmark: _Toc323128899][bookmark: _Toc331162646]

[bookmark: _Toc345918762][bookmark: _Toc345919192][bookmark: _Toc478041501]Section 9:  SWPPP Certification
(See CGP Part 9)

ITD Certification Statement
I certify under penalty of law that this document and all attachments were prepared under my direction or supervision in accordance with a system designed to assure that qualified personnel properly gathered and evaluated the information contained therein.  Based on my inquiry of the person or persons who manage the system, or those persons directly responsible for gathering the information, the information contained is, to the best of my knowledge and belief, true, accurate, and complete.  I am aware that there are significant penalties for submitting false information, including the possibility of fine and imprisonment for knowing violations.
	Name (printed)
	Title
	Signature
	Date

	
	
	
	



Prime Contractor Certification Statement
I certify under penalty of law that this document and all attachments were prepared under my direction or supervision in accordance with a system designed to assure that qualified personnel properly gathered and evaluated the information contained therein.  Based on my inquiry of the person or persons who manage the system, or those persons directly responsible for gathering the information, the information contained is, to the best of my knowledge and belief, true, accurate, and complete.  I am aware that there are significant penalties for submitting false information, including the possibility of fine and imprisonment for knowing violations.
	Name (printed)
	Title
	Signature
	Date

	
	
	
	



Additional Operator or Local Entity Certification Statement
I certify under penalty of law that this document and all attachments were prepared under my direction or supervision in accordance with a system designed to assure that qualified personnel properly gathered and evaluated the information contained therein.  Based on my inquiry of the person or persons who manage the system, or those persons directly responsible for gathering the information, the information contained is, to the best of my knowledge and belief, true, accurate, and complete.  I am aware that there are significant penalties for submitting false information, including the possibility of fine and imprisonment for knowing violations.
	Name (printed)
	Title
	Signature
	Date

	
	
	
	



Repeat as needed for additional operators at the site.  Any operator with permit coverage for this project needs to certify the SWPPP.

[bookmark: _Toc158630014][bookmark: _Toc323128900][bookmark: _Toc331162647]
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[bookmark: _Toc345918763][bookmark: _Toc345919193][bookmark: _Toc478041502]SWPPP Appendices
[bookmark: _Toc345918764][bookmark: _Toc345919194]

[bookmark: _Toc478041503]Appendix A – Site Maps 

See SWPPP Section 3.6, CGP 7.2.4 for required Site Map details.  Based on recommendations from EPA Inspectors, in addition to CGP requirements, it is recommended that the Contractor show locations of spill response and cleanup kits on the site maps. Include ITD Standard Drawings for Applicable BMPs.



[bookmark: _Toc345918765][bookmark: _Toc345919195][bookmark: _Toc478041504]Appendix B – Copy of 2022 Construction General Permit 

· Insert a copy of the 2022 CGP printed double sided or two sheets per page for space saving purposes.
[bookmark: _Toc345918766][bookmark: _Toc345919196]


[bookmark: _Toc478041505]Appendix C – Copy of NOIs and IDEQ Acknowledgement Letters from all Operators 

· Insert a copy of NOIs and IDEQ's acknowledgment letters showing coverage under the CGP

· Insert a copy of any NOTs that are filed as Operators terminate their permit coverage.



[bookmark: _Toc478041506][bookmark: _Toc345668560][bookmark: _Toc345918767][bookmark: _Toc345919197]Appendix D  - ITD Form 2951 – Contractor or Local Entity CGP Signature Authority

[bookmark: _Toc345668562][bookmark: _Toc345918769][bookmark: _Toc345919199]Follow the ITD “Form Finder” link below and search by the form number.

http://apps.itd.idaho.gov/apps/formfinder2dmz



[bookmark: _Toc478041507]Appendix E - ITD Form 2952 – ITD Delegation of CGP Signature Authority

Follow the ITD “Form Finder” link below and search by the form number.

http://apps.itd.idaho.gov/apps/formfinder2dmz



[image: ]

[bookmark: _Toc478041508]Appendix F – ITD Form 2954 - Subcontractor Certifications/Agreements

Follow the ITD “Form Finder” link below and search by the form number.

http://apps.itd.idaho.gov/apps/formfinder2dmz



[bookmark: _Toc478041509]Appendix G –ITD Form 2802, Stormwater Compliance Inspection & Inspection Instructions and Procedures

Follow the ITD “Form Finder” link below and search by the form number.

http://apps.itd.idaho.gov/apps/formfinder2dmz


[bookmark: _Toc345668563][bookmark: _Toc345918770][bookmark: _Toc345919200][bookmark: _Toc478041510]Appendix H – Completed ITD 2802, Stormwater Compliance Inspection Reports

Note:  Place an uncertified copy of each inspection report into this appendix as a placeholder until the DE/DEM certified version is routed back to the SWPPP.  The suggested turn-around time to get certified copies back into the SWPPP is 2 weeks or less. 




[bookmark: _Toc478041511]Appendix I -  ITD Form 2953 - Corrective Action Reporting Tables

Follow the ITD “Form Finder” link below and search by the form number.

http://apps.itd.idaho.gov/apps/formfinder2dmz

 


[bookmark: _Toc478041512][bookmark: _Toc345668566][bookmark: _Toc345918773][bookmark: _Toc345919203]Appendix J -  ITD Form 2955 - SWPPP Modification Log

Follow the ITD Form Finder link below and search by the form number.

http://apps.itd.idaho.gov/apps/formfinder2dmz


[bookmark: _Toc478041513]Appendix K – ITD Form 2956 - Grading and Stabilization Activities Log 

Follow the ITD Form Finder link below and search by the form number.

http://apps.itd.idaho.gov/apps/formfinder2dmz




[bookmark: _Toc478041514]Appendix L – ITD Form 2957 – SWPPP Modification and /Or Corrective Action Report

Follow the ITD Form Finder link below and search by the form number.

http://apps.itd.idaho.gov/apps/formfinder2dmz





[bookmark: _Toc478041515]Appendix M – SWPPP Training and Qualifications

Include:

· ITD Inspector qualification certificate
· Contractor’s Water Pollution Control Manager (WPCM) qualification certificate.

Use ITD Form 2958 – SWPPP Training Log to document any additional project specific training completed. 

Follow the ITD Form Finder link below and search by the form number.

http://apps.itd.idaho.gov/apps/formfinder2dmz


[bookmark: _Toc478041516]Appendix N – Endangered Species Documentation

Insert documentation consistent with SWPPP Section 4.1


[bookmark: _Toc478041517]Appendix O – Historic Properties Documentation

Not required for IPDES. Documentation optional - if available from other project development reviews.



[bookmark: _Toc345668570][bookmark: _Toc345918777][bookmark: _Toc345919207][bookmark: _Toc478041518]Appendix P – Additional Tribal, State, or Local Programs

Insert documentation consistent with SWPPP Section 4.3 and 4.4



[bookmark: _Toc345668571][bookmark: _Toc345918778][bookmark: _Toc345919208][bookmark: _Toc478041519]Appendix Q – Turbidity Monitoring Records

If applicable to this project, insert documentation consistent with SWPPP Section 3.2. and the Turbidity Monitoring contract Special Provision. Use this Appendix for Discharge Turbidity Monitoring and Dewatering Monitoring documentation. See Construction General Permit Appendix I – Suggested Format for Turbidity Monitoring Reports



[bookmark: _Toc478041520]Appendix R - ITD Form 2790 -  Notice of Potential Violation of CGP or Notice of Prohibited Discharge


Follow the ITD Form Finder link below and search by the form number.

http://apps.itd.idaho.gov/apps/formfinder2dmz
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Your Economic Opportunity Idaho Transportation Department

DATE: November 9, 2021 Program Number(s)

TO: District Engineers 1_—6 Key Number(s)

FROM: Dan McEm Program ID, County, Etc.Stormwater Permitting
Chief Operations Officer

RE: Signatory Authorization for the NPDES/IPDES General Constructon Permit

The purpose of this document is to provide authorization from the Certilying Official/Administrator (District
Engineer) in regards to the National Pollutant Discharge Elimination System Construction General Permit
(NPDES) and Idaho Pollutant Discharge Elimination System (IPDES).

Per the NPDES Construction General Permit (CGP) Appendix I, Subsection 11.1.3 the Certifying Official for
a public agency is a senior executive officer having the responsibility for the overall operations of a principal
geographic unit. For ITD's purposes the following authorizations are made:

The District Engineer is the Certifying Official for certification of the Notice of Intent and the Notice of
Termination.

In the event that the District Engineer (Certifying Official) is not available for certifying the Notice of
Intent or Notice of Termination the Acting District Engineer becomes the Certifying Official.

For the purposes of the CGP this operational procedure duly authorizes the Resident Engineer to
sign all documents except the Notice of Intent and Notice of Termination.

Itis required that this authorization document be placed in all Stormwater Pollution Prevention Plans
(SWPPPs) and available to the Environmental Protection Agency and the Idaho Department of
Environmental Quality upon request.

Cc: Highways Development Administrator
Highways Construction & Operations Administrator
Environmental Services Manager




