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ITD 0912   (Rev. 10-03)
Steel Bars For Concrete Reinforcement

Work Sheet

	Date Received in Lab
	Lab Number
	Through

	     
	     
	     

	Key Number
	Project Number
	County

	     
	     
	     

	Contract Item Number
	Date Sampled
	Sampled By

	     
	     
	     

	Identification Number
	Steel Mill Name
	Steel Fabricator
	Steel Grade

	     
	     
	     
	     


	Heat Number
	     
	     
	     
	     
	     
	     
	Specifications

 FORMCHECKBOX 
 ASTM A 615 

 FORMCHECKBOX 
 AASHTO M 31

	Bar Number
	     
	     
	     
	     
	     
	     
	

	Length, ft.
	     
	     
	     
	     
	     
	     
	

	Length, in.
	     
	     
	     
	     
	     
	     
	

	Weight, lb.
	     
	     
	     
	     
	     
	     
	

	Unit Weight, lb/ft
	     
	     
	     
	     
	     
	     
	Individual Bar 6% Min. Under Wt

	Theor. Unit Weight, lb/ft
	     
	     
	     
	     
	     
	     
	

	X Sectional Area, sq in
	     
	     
	     
	     
	     
	     
	

	Yield Point, lb.
	     
	     
	     
	     
	     
	     
	

	Yield Point, lb/sq in.
	     
	     
	     
	     
	     
	     
	Grd 40 = 40,000
Grd 60 = 60,000 
Grd 75 = 75,000

	Tensile 
Strength, lb.
	     
	     
	     
	     
	     
	     
	

	Tensile Strength, lb/sq in
	     
	     
	     
	     
	     
	     
	Grd 40 = 70,000
Grd 60 = 90,000 

Grd 75 = 100,000

	Elongation in 8 inches, %
	     
	     
	     
	     
	     
	     
	

	Fracture
	     
	     
	     
	     
	     
	     
	

	Cold Bend
	     
	     
	     
	     
	     
	     
	Without Cracking


	Remarks

	     

	Tested By
	Computed By
	Checked By

	
	
	


PSI, Min





PSI, Min





}





}
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