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	Emulsified Asphalt and Cutbacks	itd.idaho.gov
	One Grade and One Source Only per Sheet

	Emulsified asphalt for seal coat, road mix, or scrub coat and cutbacks:	Sample from each compartment, each supplier, and each
grade of asphalt.
Diluted emulsified asphalt for tack coat, prime coat, or fog seal:	Sample before asphalt has been diluted!
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[bookmark: Check4]|_| Check here if these samples are the last samples for this project.  If possible, notify the central laboratory at extension 8454.
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Please submit the original form ITD 1045 with the samples. 
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