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ITD 1813   (Rev. 7-07)
Report Of Tests On Uncoated Seven-Wire
itd.idaho.gov 
Stress Relieved Strand For Prestressed Concrete

	Lab Number
	     

	

	Key Number
	Project Number
	Project Name
	Contract Item Number

	     
	     
	     
	     

	Identification Number (Program/Task/Phase/Sample #
	Date Sampled
	Sampled By
	WAQTC Number
	Qty Represented

	     
	     
	     
	     
	     

	Send Report To
	Address/Location
	Date Lab Received
	Date Tested

	     
	     
	     
	     

	Heat Number
	Reel or Pack Number
	Material Source

	     
	     
	     


	Specifications – ASTM A 416

	Size:
	 FORMCHECKBOX 
 0.500
 FORMCHECKBOX 
 0.600
 FORMCHECKBOX 
 Standard 270 k
 FORMCHECKBOX 
 Mini-Lax 270 k

	

	Test Results

	Identification Number
	     
	     
	     
	
	Specifications

	Diameter of Strand, in.
	     
	     
	     
	
	     
	
	+0.026
	

	
	
	
	
	
	     
	
	-0.006
	

	Diameter of Outer Wire, in.
	     
	     
	     
	
	     
	
	Min. Diff. Between Center and Outer Wire

	Diameter of Center Wire, in.
	     
	     
	     
	
	
	
	

	Area of Strand, sq. in.
	     
	     
	     
	
	Nom.

	Yield Strength, lbs.
	     
	     
	     
	
	Min.

	Tensile Strength, lbs.
	     
	     
	     
	
	Min.

	% Elongation in 24”
	     
	     
	     
	
	3.5% Min.

	Modulus of Elasticity –X(106)
	     
	     
	     
	
	

	

	Remarks

	     

	Material as represented is:
	 FORMCHECKBOX 
 Acceptable
	 FORMCHECKBOX 
 Subject to Rejection

	
	
	
	
	

	This report covers only material as represented by the sample submitted.

	Tested By
	Date Mailed
	Materials Engineer’s Signature

	     
	     
	     
	, P.E.


